

[bookmark: _uf8mursmvlpa]BulletCam HL (5 Mp/2.8 mm)

[bookmark: _vmwa67u82o74]Wired AI-powered security IP camera with a 110° viewing angle, hybrid illumination, TrueWDR, microphone, and PoE/12 V. For outdoor and indoor use.
	[bookmark: _tcapln3ynkt7]Camera
	[bookmark: _eutdtssqb9vh]Image sensor
5 MP CMOS, 1/2.8" type
[bookmark: _tca3xp6v47xp]Lens focal length
2.8 mm
[bookmark: _ot142q734bpn]Maximum aperture
f/1.6
[bookmark: _cyhkhgq4b2rg]Lens iris type
fixed
[bookmark: _5e6tox1iuhpe]Lens focal type
fixed
[bookmark: _fkm3n2m9c2ly]Field of view
horizontal: 100–110°
vertical: 50–60°
diagonal: 125–135°
[bookmark: _92l7y4s1j7zl]DORI distance
· Detection: 65 m
· Observation: 26 m
· Recognition: 13 m
· Identification: 6.5 m
[bookmark: _b8yu8bajgkbu]Maximum illumination distance
· white LED: up to 50 m
· IR LED: up to 50 m
Intelligent lighting control automatically adjusts the intensity of IR and white LEDs in real time to prevent overexposure. This ensures clear visibility of objects at varying distances — whether close to or far from the camera — in low-light conditions.
[bookmark: _m3fne1whdl3e]Minimum illumination
color: 0.005 lx
B/W: 0 lx
[bookmark: _oapwfjlz9jr3]Signal-to-noise ratio (SNR)
more than 52 dB

	[bookmark: _jg92tzc9atgl]Video
	[bookmark: _96hum32ia6e1]Resolution
· 5 MP (2880 × 1620)
· 4 MP (2560 × 1440)
· 3 MP (2304 × 1296)
· 2 MP (1920 × 1080)
· 0.6 MP (1024 × 576)
[bookmark: _s6cck7sff449]Frame rate
up to 25 fps
[bookmark: _sd12mdwi2u9x]Image rotation
0°, 180°
[bookmark: _trvbdegj4lsw]Video codec
H.265, H.264
[bookmark: _h6122fqx68ap]Dynamic range
120 dB (True WDR)
[bookmark: _sajfqzfx3pqt]Storage
microSD
The camera supports microSD up to 256 GB. The memory card should be Class V30 or faster. The card is not included in the complete set.

	[bookmark: _f6dvsvkangau]Audio
	Built-in microphone
With the corresponding settings, the camera can record audio at the scene.

Audio codec
G711-ULAW, G711-ALAW, G726, G722

	[bookmark: _ehr467ongxnb]Intelligent video analytics
	Motion detection
The camera detects motion using software image frame analysis.

AI object detection
People
Pets
Vehicles

	[bookmark: _21zafklh9bw3]Network
	[bookmark: _sszcrnyefq1f]Port
1 × RJ-45 self-adaptive Ethernet (10/100 Mbps)
[bookmark: _wusweuluuwfn]Protocol
HTTP, HTTPS, TCP/IP, IPv4, RTSP, UDP, DHCP, DNS
[bookmark: _osfex03s6gwd]ONVIF®
conformant with ONVIF® Profile G and S
The device implements ONVIF® H.265 (HEVC) encoding, transmission of motion detection and AI recognition events, control over Wide Dynamic Range (WDR), and other image settings — not ONVIF® profile or add-on conformant.

	[bookmark: _5dkl2054ksx0]Key features
	[bookmark: _be07vy8u6mex]Video protocol
JetSparrow
Fast and encrypted peer-to-peer video protocol developed by Ajax Systems.
[bookmark: _9oe1d4jyjgtl]Visual verification of Ajax alarms
The system allows you to configure a scenario according to which Ajax detectors trigger selected cameras to start recording. The recorded event is immediately delivered to the mobile or desktop monitoring app.
[bookmark: _j4gadut6dku7]Privacy
Advanced privacy controls ensure a high level of personal data protection. All access rights — including those for mobile app users, installers, and monitoring company operators via Ajax PRO Desktop — are fully configurable by the device owner. This guarantees that only authorized parties can access video streams, event history, or device settings, in accordance with the owner’s preferences.

	[bookmark: _66i67huf9nhc]Sabotage protection
	[bookmark: _o5dgwbp28rbw]mTLS
Encrypted connection for data protection.
[bookmark: _cintnrn1s8ua]Authentication
via Ajax Cloud
[bookmark: _s5f2oyjhw06r]Secure Boot
Protection against firmware spoofing.
[bookmark: _y42ygziaazh1]OTA signature verification
Secure automatic firmware update.

	[bookmark: _k86pndlhd2mx]Power supply
	[bookmark: _e3sg5m64cmni]PoE standard
802.3at/af
[bookmark: _r5e2ibte23gl]PoE power consumption
· maximum: up to 7.3 W
· average: up to 6.0 W
[bookmark: _ccewq3ze8w8h]Power supply unit
12 V⎓ ± 20%, 1 А
[bookmark: _81b7a5uv93ge]12 V DC power consumption
· maximum: up to 6.3 W
· average: up to 5.1 W

	[bookmark: _5cuo19vcib7x]Enclosure
	Dimensions
198 × 76 × 76 mm
7.78″ × 2.99″ × 2.99″

Weight
550 g
1.21 lb

Operating temperature range
from −30 °C to +60 °C
from −22 °F to 140 °F

Operating humidity
up to 90%

Protection class
IP65, IK08

	[bookmark: _jfndqvwvzllu]Color
	Black
White



	[bookmark: _jfndqvwvzllu]Complete set
	BulletCam HL (5 Mp/2.8 mm)
Installation template
Installation kit
Quick start guide

	Warranty
	24 months





