

[bookmark: _mnh9pcvmd11c]BulletCam HL (8 Mp/2.8 mm)

[bookmark: _3le7audwvrdp]Wired AI-powered security IP camera with a 110° viewing angle, hybrid illumination, TrueWDR, microphone, and PoE/12 V. For outdoor and indoor use.
	[bookmark: _bwnnuavqybdf]Camera
	Image sensor
8 MP CMOS, 1/2.7" type
Lens focal length
2.8 mm
Maximum aperture
f/1.6
Lens iris type
fixed
Lens focal type
fixed
Field of view
· horizontal: 100–110°
· vertical: 50–60°
· diagonal: 125–135°
DORI distance
· Detection: 90 m
· Observation: 36 m
· Recognition: 18 m
· Identification: 9 m
Maximum illumination distance
· white LED: up to 50 m
· IR LED: up to 50 m
Intelligent lighting control automatically adjusts the intensity of IR and white LEDs in real time to prevent overexposure. This ensures clear visibility of objects at varying distances — whether close to or far from the camera — in low-light conditions.
Minimum illumination
color: 0.005 lx
B/W: 0 lx
Signal-to-noise ratio (SNR)
more than 52 dB

	[bookmark: _r38q949br653]Video
	Resolution
· 8 MP (3840 × 2160)
· 6 MP (3072 × 1728)
· 5 MP (2592 × 1944)
· 5 MP (2944 × 1656)
· 5 MP (2880 × 1620)
· 4 MP (2560 × 1440)
· 3 MP (2304 × 1296)
· 2 MP (1920 × 1080)
· 0.6 MP (1024 × 576)
Frame rate
up to 20 fps
Image rotation
0°, 180°
Video codec
H.265, H.264
Dynamic range
120 dB (True WDR)
Storage
microSD
The camera supports microSD up to 256 GB. The memory card should be Class V30 or faster. The card is not included in the complete set.

	[bookmark: _hyydgwy0q0wl]Audio
	Built-in microphone
With the corresponding settings, the camera can record audio at the scene.

Audio codec
G711-ULAW, G711-ALAW, G726, G722

	[bookmark: _szh395yhqprx]Intelligent video analytics
	Motion detection
The camera detects motion using software image frame analysis.

AI object detection
People
Pets
Vehicles

	[bookmark: _7falgygafq0h]Network
	[bookmark: _sszcrnyefq1f]Port
1 × RJ-45 self-adaptive Ethernet (10/100 Mbps)
[bookmark: _wusweuluuwfn]Protocol
HTTP, HTTPS, TCP/IP, IPv4, RTSP, UDP, DHCP, DNS
[bookmark: _osfex03s6gwd]ONVIF®
conformant with ONVIF® Profile G and S
The device implements ONVIF® H.265 (HEVC) encoding, transmission of motion detection and AI recognition events, control over Wide Dynamic Range (WDR), and other image settings — not ONVIF® profile or add-on conformant.

	[bookmark: _fdynrgnnjhay]Key features
	[bookmark: _be07vy8u6mex]Video protocol
JetSparrow
Fast and encrypted peer-to-peer video protocol developed by Ajax Systems.
[bookmark: _9oe1d4jyjgtl]Visual verification of Ajax alarms
The system allows you to configure a scenario according to which Ajax detectors trigger selected cameras to start recording. The recorded event is immediately delivered to the mobile or desktop monitoring app.
[bookmark: _j4gadut6dku7]Privacy
Advanced privacy controls ensure a high level of personal data protection. All access rights — including those for mobile app users, installers, and monitoring company operators via Ajax PRO Desktop — are fully configurable by the device owner. This guarantees that only authorized parties can access video streams, event history, or device settings, in accordance with the owner’s preferences.

	[bookmark: _pn8vv3mne5em]Sabotage protection
	[bookmark: _o5dgwbp28rbw]mTLS
Encrypted connection for data protection.
[bookmark: _cintnrn1s8ua]Authentication
via Ajax Cloud
[bookmark: _s5f2oyjhw06r]Secure Boot
Protection against firmware spoofing.
[bookmark: _y42ygziaazh1]OTA signature verification
Secure automatic firmware update.

	[bookmark: _fm920lniuyg5]Power supply
	[bookmark: _16a6zqm7rz6n]PoE standard
802.3at/af
[bookmark: _wgdm9ptgm2ql]PoE power consumption
· maximum: up to 8.1 W
· average: up to 7.0 W
[bookmark: _fynvsvacbfcr]Power supply unit
12 V⎓ ± 20%, 1 А
[bookmark: _x3tfr3xdf59v]12 V DC power consumption
· maximum: up to 7.0 W
· average: up to 6.0 W

	[bookmark: _j1kbx3eepxna]Enclosure
	Dimensions
198 × 76 × 76 mm
7.78″ × 2.99″ × 2.99″

Weight
550 g
1.21 lb

Operating temperature range
from −30 °C to +60 °C
from −22 °F to 140 °F

Operating humidity
up to 90%

Protection class
IP65, IK08

	[bookmark: _jfndqvwvzllu]Color
	Black
White


	[bookmark: _jfndqvwvzllu]Complete set
	BulletCam HL (8 Mp/2.8 mm)
Installation template
Installation kit
Quick start guide

	Warranty
	24 months





